* Settings
  + CVM
  + Data Logger
  + Interface
  + Load controller
  + Process controller
    - Fetch settings
    - TC\_low\_temp\_threshold
    - TC\_high\_temp\_ threshold
    - TC\_high\_temp\_ threshold \_warning\_buffer
    - P\_sig\_flags
    - HIH6120\_address[8]
    - HIH6120\_flags = 0;
    - HIH\_interval = 50;
    - t H2N2\_flag = 0;
    - Cathode\_target\_T = 77.0;
    - Cathode\_T\_Hysteresis = 1;
    - t Pressure\_sensor\_minimum\_thresh
    - t Cathode\_flow\_sensor\_minimum\_th
    - CTHD\_FLW\_stoich = 2;
    - \_t CTHD\_FLW\_min = 65;
    - Coolant\_T\_target = 72;
    - Coolant\_T\_Hysteresis = 1;
    - Coolant\_high\_temp\_thresh = 80;
    - Coolant\_high\_temp\_warning\_buffe
  + Safety controller